# 9442_r

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: Graphic Services Unit
      Originator: Natural Resource Information Management
      Originator: Resource Condition and Trend Group
      Originator: Natural Resource Sciences
      Publication_Date: July 2004
      Title: 9442_r
      Geospatial_Data_Presentation_Form: vector digital data
      Series_Information:
        Series_Name: Geoscience Data, Queensland Mapping Data (GEOLDATA)
        Issue_Identification: July 2004
      Publication_Information:
        Publication_Place: Brisbane, Australia
        Publisher: Department of Natural Resources, Mines and Energy
      Online_Linkage:
        \\NCH52600\D\GEOLDATA_CDS_JULY04\ZONE56S\IPSWICH_9442\Esri Shape\9442_r.shp
  Description:
    Abstract:
      The polygons in this dataset are a digital representation of the distribution or extent of geological units within the area. Polygons have a range of attributes including unit name, age, lithological description and an abbreviated symbol for use in labelling the polygons. These have been extracted from the Rock Units Table held in the Department of Natural Resources, Mines and Energy Merlin Database.
    Purpose:
      To display the geology polygons which define the extent of rock units.
    Supplemental_Information:
      Data captured at 1:25 000 scale. The data set is sourced from the Department's Geoscience and Resources Database (GRDB), a component of the Mineral and Energy Resources Location and Information Network (MERLIN) corporate database.(GRDB), a component of the Mineral and Energy Resources Location and Information Network (MERLIN) corporate database.

      NOTE: GEOLDATA was in most cases compiled based on Datum AGD66. The map tile coverages so compiled have now been projected to geographics based on Datum GDA94. Consequently the boundaries for these map tiles will not conform to the Latitude and Longitude graticule based on Datum GDA94.

  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 2004 July
    Currentness_Reference: publication date
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: 152.501067
      East_Bounding_Coordinate: 153.001064
      North_Bounding_Coordinate: -27.498393
      South_Bounding_Coordinate: -27.998421
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: geoscientificInformation
      Theme_Keyword: GEOSCIENCES Geology
      Theme_Keyword: Geology maps
      Theme_Keyword: Geology mapping
    Place:
      Place_Keyword_Thesaurus: ANSLIC GEN
      Place_Keyword: Queensland
  Access_Constraints:
    The Department licenses all digital data and products, whether there is a fee charged or not. The information sheet on the Department's website provides an overview of the different licences available. <http://www.nrme.qld.gov.au/products/access_pricing/licence.html> The Department only enters into sharer agreements where there is mutual benefit and these must be approved by the Deputy Director General, Natural Resource Services. This data is provided under a User Licence- refer to website as above, and follow the links to User Licence. To request provision of the data under any other licenses described on this website, a written request must be made to the Department.
  Use_Constraints:
    The data are supplied under a User Licence for non-commercial purposes for internal use only, and must not be sold or distributed to any third party. Refer to web address: <http://www.nrme.qld.gov.au/products/access_pricing/licences/user_info.html> A sample User Licence is available in <http://www.nrme.qld.gov.au/products/access_pricing/pdfs/sample_user_licence_v1_2.pdf> With reference to the "Methods of Acknowledging Agreement"; in 4.1- you must register at www.nrme.qld.gov.au/products so you can be advised of updates to the data.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Ian Withnall
        Contact_Organization: Department of Natural Resources, Mines & Energy
      Contact_Position: Senior Geoscientist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: Natural Resource Sciences
        Address: Block A
        Address: 80 Meiers Road
        Address: Indooroopilly
        City: Brisbane
        State_or_Province: QLD
        Postal_Code: 4068
        Country: Australia
      Contact_Voice_Telephone: +61 7 3362 9363
      Contact_Facsimile_Telephone: +61 7 3362 9343
      Contact_Electronic_Mail_Address: ian.withnall@nrm.qld.gov.au
      Hours_of_Service: 9.00 AM - 4.00PM MON- FRI
  Data_Set_Credit:
    Geology by: 1970-1973; L C Cranfield; 1975-1977; L C Cranfield, D Trezise, L J Hutton, PM Green
  Native_Data_Set_Environment:
    Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 4; ESRI ArcCatalog 8.3.0.800

Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report:
      Geological units (and their boundaries) and other linear structures such as faults and folds were largely interpreted from aerial photographs. More recently (since the mid-90s) geophysical datasets have played an increasingly significant part in the interpretation. This interpretation is carried out in conjunction with numerous field observations and or measurements, and sample collection and analysis. The location of sites in the Geological Site Database available from the Department of Natural Resources, Mines and Energy (and extracted from its MERLIN corporate database) gives an indication of the level of fieldwork undertaken for mapping carried out since 1986.
  Completeness_Report:
    Completeness and consistency of classification needs to be considered in the context of the time span of the source mapping and the highly interpretive nature of the discipline. Although broadly similar classification and measurement techniques have been applied to geological map compilation by geological surveys for many years, resultant data tends to reflect individual geologists' ideas and preferences. For example the classification of boundaries, faults and similar features (ranging from approximate, concealed, inferred) is not particularly consistent and needs to be treated with caution. There is no consistent record of the extent of field observation as opposed to air-photo interpretation, but location of sites in the Geological Site Database available from the Department of Natural Resources, Mines and Energy (and extracted from its MERLIN corporate database) gives an indication of the level of fieldwork undertaken for mapping carried out since 1986.
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report:
        An accurate assessment of the horizontal accuracy is not possible, because the history of the original source information of each line and subsequent revisions are not fully known. Apart from uncertainties in interpretation and location of these features on the ground or on various images, other errors can result from inaccurate topographic bases, spheroid or datum differences, map compilation processes and subsequent digitising. This dataset was compiled on photo-overlays on unrectified aerial photographs ranging from 1:25000 to 1:85000 scale. Maps were compiled from these overlays onto topographic bases, using drainage and cultural features for spatial control. Assuming the feature had been correctly interpreted and located on the aerial photographs, the estimated positional error is estimated at 1mm at the respective scale. To that could be added at least another 1mm due to misfits between the air-photo and the base because of distortion in the photograph or inaccuracies in the base. Therefore, at best, the total positional error due to map production processes is about +/- 170m from 1:85000-scale photographs and +/- 50m from 1:25000 scale. It is stressed that this does not take into account the uncertainties in interpretation and location of these features mentioned above, so that the actual error is often much greater than listed.
  Lineage:
    Process_Step:
      Process_Description: Metadata imported.
      Source_Used_Citation_Abbreviation: C:\data\test\testmeta\template_r.shp.xml
    Process_Step:
      Process_Description: Metadata imported.
      Source_Used_Citation_Abbreviation: D:\GEOLDATA_CD_COVERAGE\meta_templates\template_r.shp.xml

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 1036

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Geographic:
      Latitude_Resolution: 0.000000
      Longitude_Resolution: 0.000000
      Geographic_Coordinate_Units: Decimal degrees
    Geodetic_Model:
      Horizontal_Datum_Name: D_GDA_1994
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: 9442_r
      Entity_Type_Definition:
        Polygons have a range of attributes including unit name, age, lithological description and an abbreviated symbol for use in labelling the polygons.
      Entity_Type_Definition_Source:
        The Rock Units Table held in the Department of Natural Resources, Mines and Energy Merlin Database.
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain:
          Sequential unique whole numbers that are automatically generated.
      Beginning_Date_of_Attribute_Values: March 2004
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: KEY
      Attribute_Definition: Unique polygon identifier and relate item for poygon attributes
    Attribute:
      Attribute_Label: ROCK_U_NAM
      Attribute_Definition:
        The Map Unit Name of the polygon. In the case of named units it comprises of the standard binomial name. Unnamed subdivisions of named units include the binomial name with a letter symbol as a suffix. Unnamed units are represented by a letter symbol, usually in combination with a map sheet number.
    Attribute:
      Attribute_Label: AGE
      Attribute_Definition: Geological age of unit
    Attribute:
      Attribute_Label: LITH_SUMMA
      Attribute_Definition:
        Provides a brief description of the map units as they have been described in the course of the project work, or as has appeared on relevant hard copy map legends.
    Attribute:
      Attribute_Label: ROCK_U_TYP
      Attribute_Definition:
        Provides a means of separating map units, eg for constructing a map reference. This item will contain one of the following: STRAT- Stratigraphic unit, including sedimentary, volcanic and metamorphic rock units. INTRU- Intrusive rock units; COMPST- Compound unit where the polygon includes two or more rock units, either stratigraphic, intrusive or both; COMPST- Compound unit, as above where the dominant or topmost unit is of the STRAT type; COMPIN- Compound unit, as above, where the dominant unit is of the INTRU type; WATER- Water bodies- Large dams, lakes, waterholes.
    Attribute:
      Attribute_Label: SEQUENCE_N
      Attribute_Definition:
        A numeric field to allow sorting of the rock units in approximate stratigraphic order as they would appear on a map legend.
    Attribute:
      Attribute_Label: DOMINANT_R
      Attribute_Definition:
        A simplified lithological description to allow generation of thematic maps based on broad rock types.
    Attribute:
      Attribute_Label: MAP_SYMBOL
      Attribute_Definition:
        Provides an abbreviated label for polygons. Mostly based on the letter symbols as they appear on published maps or the original hard copy compilation sheets. These are not unique across the State, but should be unique within a single map tile, and usually adjacent tiles.
    Attribute:
      Attribute_Label: NAME_100K
      Attribute_Definition: Name of 1:100 000 map sheet coincident with the data extent.
  Overview_Description:
    Entity_and_Attribute_Overview:
      Polygon Attribute information includes Polygon Key, Rock Unit Name, Age, Lithology, Rock Unit Type, Map Symbol and 1:100 000 sheet name.

Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Department of Natural Resources, Mines and Energy
      Contact_Position: Sales and Information Centre
      Contact_Voice_Telephone: +61 7 3237 1431
      Contact_Facsimile_Telephone: +61 7 3221 9517
      Contact_Electronic_Mail_Address: sales@nrm.qld.gov.au
      Hours_of_Service: 8:30 AM - 4:30 PM AEST MON - FRI
  Resource_Description: GEOSCIENCE DATA Queensland Mapping Data GEOLDATA CD
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 2.415
    Fees:
      Access fee- Refer to <http://nrm.dnr.qld.gov.au/products/cat_services.php?category=537&description=Digital+geoscience+data>
    Ordering_Instructions:
      Phone, fax or email request to Information and Sales. Payment by credit (processed by Sales), cheque or Bank transfer prior to postage of data.

Metadata_Reference_Information:
  Metadata_Date: 20040625
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization:
          Graphic Services Unit- Department of Natural Resources, Mines and Energy
        Contact_Person: Peter Goldsworthy
      Contact_Position:
        Spatial Information Resource- Information Management Authority for GEOLDATA
      Contact_Address:
        Address_Type: mailing address
        Address: Natural Resource Sciences
        Address: Block C , Level 3
        Address: 80 Meiers Road
        Address: Indooroopilly
        City: Brisbane
        State_or_Province: QLD
        Postal_Code: 4068
        Country: AUSTRALIA
      Contact_Voice_Telephone: 61 7 3896 9810
      Contact_Facsimile_Telephone: 61 7 3896 9782
      Contact_Electronic_Mail_Address: peter.goldsworthy@nrm.qld.gov.au
      Hours_of_Service: 9:00 AM- 4:00 PM AEST MON- FRI
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.7.33 on Fri Jun 25 11:13:27 2004