Great Artesian Basin

DATA DICTIONARY

Birkhead Walloon aquitard

June 2014

Ransom G, Stewart G, Ransley T, and Bell J.

Geoscience Australia

The data referred to in this data dictionary can be obtained from Geoscience Australia at www.ga.gov.au

**Publication details:**

[](http://creativecommons.org/licenses/by/3.0/au/)  
© Commonwealth of Australia (Geoscience Australia) year of publication.

This product is released under the Creative Commons Attribution 3.0 Australia Licence.

<http://creativecommons.org/licenses/by/3.0/au/deed.en>

### Birkhead Walloon aquitard extents

**File name/s** AdoriSpringBok\_Aquifer\_Extent

**Type** Vector: ESRI shapefile

**Scale** 1:1 000 000

**Projection** Lambert conformal conic GDA 1994, with central meridian 134 degrees longitude, standard parallels at -18 and -36 degrees latitude.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Value | Type | Compulsory | Valid Values | Description | Rules |
| name | String, 100 | Yes | Name of the aquifer or aquitard | Name of aquifer or Aquitard |  |
| descript | String, 254 | Yes | Great Artesian basin regional hydrogeology | Description of purpose of the data |  |

### 

### Birkhead Walloon aquitard outcrop

**File name/s** AdoriSpringBok\_Aquifer\_Outcrop

**Type** Vector: ESRI shapefile

**Scale** 1:1 000 000

**Projection** Lambert conformal conic GDA 1994, with central meridian 134 degrees longitude, standard parallels at -18 and -36 degrees latitude.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Value | Type | Compulsory | Valid Values | Description | Rules |
| name | String, 100 | Yes | names of GAB aquifers and aquitards | Name of aquifer or aquitard outcrop |  |
| descript | String, 254 | Yes | Great Artesian basin regional hydrogeology | Description of data |  |

### Birkhead Walloon aquitard thickness isopachs

**File name/s** AdoriSpringBok\_Aquifer\_Isopach

**Type** Vector: ESRI shapefile

**Scale** 1:1 000 000

**Projection** Lambert conformal conic GDA 1994, with central meridian 134 degrees longitude, standard parallels at -18 and -36 degrees latitude.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Value | Type | Compulsory | Valid Values | Description | Rules |
| name | String, 100 | Yes | name of the GAB aquifer or aquitard that this data belongs to | Name of the aquifer or aquitard |  |
| descript | String,  254 | Yes | Great Artesian basin regional hydrogeology | Description of purpose of the data. |  |
| isopach | Numeric | Yes |  | Isopach thickness |  |

### Birkhead Walloon aquitard thickness data point locations

**File name/s** AdoriSpringBok\_Aquifer\_DataPoints

**Type** Vector: ESRI shapefile

**Scale** 1:1 000 000

**Projection** Lambert conformal conic GDA 1994, with central meridian 134 degrees longitude, standard parallels at -18 and -36 degrees latitude.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Value | Type | Compulsory | Valid Values | Description | Rules |
| name | String, 100 | Yes | name of the GAB aquifer or aquitard that this data belongs to | Name of the aquifer or aquitard |  |
| descript | String,  254 | Yes | Great Artesian basin regional hydrogeology | Description of purpose of the data. |  |
| lat | Numeric | Yes | Valid Latitudes | Latitude location of data point (GCS GDA 1994) |  |
| long | Numeric | Yes | Valid Longitudes | Longitude location of data point (GCS GDA 1994) |  |