# Cadastral data fortnightly extract Flinders Local Government Area

## Identification

Title: Cadastral data fortnightly extract Flinders Local Government Area
Alternative title: IQATLAS.QLD_CADASTRETENURE_DCDB_CUR?LAC=3200
Date: 2014-01-12 (publication)
Online resource:
URL/service: Function: download

## Description

Abstract / Description:
The cadastral dataset is the spatial representation of property boundaries and descriptions in the above local government area. It is a fundamental reference layer for spatial information systems in Queensland. This is a complete extract from the digital cadastral database (DCDB). A lite version of the DCDB is available from the Queensland Government Information Service website. Attributes are described in the "QIF file specifications" at http://www.nrm.qld.gov.au/property/mapping/dcdata/index.html#data_attributes .
Resource format:
Name/identifier: SHP or TAB
Version: 1
Environment description:
ARCSDE
Additional Information:
In 2014 this cadastre will be extracted on the following dates and the data will be available for download within the next five working days from these dates. January 12 and 26 - February 9 and 23 - March 9 and 23 - April 6 and 20 ? May 4 and 18 - June 1, 15 and 29 - July 13 and 27 - August 10 and 24 - September 7 and 21 - October 5 and 19 - November 2, 16 and 30 - December 14 and 28. In 2015 the 1st release date will be January 11.
Language: eng
Character set: unknown

## Topic

ISO topic category codes: planningCadastre
Theme keywords:
Thesaurus: ANZLIC Search Words
Keyword: LAND-Cadastre
Date: unknown

## Spatial Data Information

Spatial representation type: vector
Coordinate Reference System EPSG code: EPSG:4283
Title: EPSG Geodetic Parameter Dataset
Date: 2007-07-16 (revision)
Edition: Version 6.13

## Contacts

Point of contact:
Organisation: Department of Natural Resources and Mines
Position: Senior Products Officer
Address:
Email: SIProductdelivery@dnrm.qld.gov.au
Phone:
Voice: 617 3896 3162
Custodian:
Organisation: Department of Natural Resources and Mines
Position: Executive Director, Land and Spatial Information
Online resource:
URL/service: http://www.derm.qld.gov.au/property/mapping/dcdata/
Owner:
Organisation: Department of Natural Resources and Mines
Position: Executive Director, Land and Spatial Information
Distributor:
Organisation: Department of Natural Resources and Mines
Position: opendata@dnrm.qld.gov.au

## Status

Progess status: completed
Maintenance and update frequency: fortnightly

## Data / Resource Constraints

Resource Access Level:
Security classification (ISO 19115): unclassified
Copyright: (as use constraint)
© State of Queensland (Department of Natural Resources and Mines) 2014
Licence: (as use constraint)
This material is licensed under a Creative Commons - Attribution 3.0 Australia licence.
The Department of Natural Resources and Mines requests attribution in the following manner:
© State of Queensland (Department of Natural Resources and Mines) 2014. Updated data available at http://dds.information.qld.gov.au/dds/.

## Temporal and Spatial extents:

Extent group:
Temporal extent:
Start: 1983-06-01 End: 2012
Bounding box:
West bounding longitude: 143.236
East bounding longitude: 145.688
South bounding latitude: -22.211
North bounding latitude: -19.568
Bounding polygon: <Polygon id="boundingInclusiveExteriorPolygon1" srsName="urn:ogc:def:crs:EPSG:6.6:4326"> <exterior> <LinearRing> <posList srsDimension="2"> -19.57 143.24 -19.57 145.69 -22.21 145.69 -22.21 143.24 -19.57 143.24</posList> </LinearRing> </exterior> </Polygon>

## Data Quality

Data quality scope:
Level: dataset
Completeness (omission):
The capture over the whole of the State is ongoing.
Consistency (conceptual):
The current DCDB can be considered as a seamless map of the State and consists of base cadastral parcels, strata level parcels (secondary interests), volumetric and easement parcels. Base parcels are contiguous with surrounding base parcels. The graphic package and the routines that extract and reload update data to the database has a tolerance of 2mm.
Positional accuracy (external, absolute):
Positional accuracy values have been allocated to all parcels in the Digital Cadastral Database (DCDB) and are an attribute of the parcel. This value reflects 'maximum error' status of the parcel and has been derived from the capture process or assigned as the DCDB data has been upgraded. The data is sourced from: Upgrade Adjustment and Upgrade Satellite Imagery.
Attribute accuracy (non quantitative):
Each polygon in the DCDB has a unique identifier called a segment-parcel number. The attributes are attached to each polygon in the DCDB based on the polygon centroid which is the segment-parcel number: Accuracy code, Centroid value, Coverage code, Excluded area value, Feature name, Linestyle code, Local Government code, Locality code, Locality name, Lot area value, Lot number, Maximum error value , Parcel indicator code, Parcel type code, Parcel number, Parcel corner value, Parcel count value, Parish code, Plan number, Segment number, Surveyed indicator, Tenure code, Update number, Update type code. The estimated accuracy of the attribute information is 98%, this is exclusive of locality and parish information.

### History:

Lineage statement:
The DCDB was captured by digitising the best available cadastral mapping at a variety of scales and map accuracies. These mapping scales ranged from Standard 1:2500 to 1:250000, Provisional 1:2500 to 1:253400 and mapping such as Parish, Locality, Environ and Town maps. At the initial capture, existing control identified from the Survey Control Database, standard cadastral and topographic mapping, photogrammetric and orthophoto compilations and this control was used as part of the digitising process. Additional control was requested if necessary. The DCDB is continuously updated by inputting metes and bounds descriptions from registered plans of subdivision and from any attribute updates from government gazettes and other administrative notifications. The DCDB is being upgraded for an improved positional accuracy, this is an ongoing process. In October 2000, the datum of DCDB was converted from AGD84 values. A distortion model based on a Queensland grid was used in the transformation process for the conversion of the DCDB co-ordinate values from AGD84 to GDA94. The distortion grid used is QLD_0900.gsb. The DCDB includes polygons and feature names for parts of the sea adjoining the coastline of Queensland. The spatial representation of any part of the sea has been delineated in the DCDB by the construction of polygons. The feature names assigned to those polygons have been obtained from a variety of sources, Topographic Maps, Navigation Charts, local usage, etc. Indeterminable Extent, the delineation in the DCDB of the extent of any part of the sea by the creation of construction lines for each polygon is to permit the inclusion of the feature name only. The construction lines are not warranted to be the actual boundaries of any water feature or to be accurate or complete.
Process step:
The DCDB data, in DCDB transfer format (IFO), is FTP'd to the Spatial Information Resource server every fortnight where it is transformed into the Spatial Information Resource (SIR) ArcSDE Geodatabase.Note: the MapInfo dataset was generated/transformed/derived from the ARCSDE dataset.

## Distribution

Format(s):
Name/identifier: Queensland Government Information Service
Specification: Download Service
Resource provider:
Organisation: Department of Natural Resources and Mines
Online resource:
URL/service: http://dds.information.qld.gov.au/dds/
Ordering information:
Fees: IncPrice=0; GST=0; Currency=AUD; AcctRef=9311662180988
Instructions: This data is available through the Queensland Government Information Service web site. Large orders over the limit are burnt to DVD and posted. An additional fee applies for postage and handling.
Format(s):
Name/identifier: downloadableData
Version: 10.0
Specification: ESRI ArcGIS Server Geoportal Extension Content Type
Distributor:
Distributor:
Organisation: Department of Natural Resources and Mines
Position: opendata@dnrm.qld.gov.au
Format(s):
Name/identifier: Through Queensland Government Information Service available as ESRI Shape file and MapInfo Tabfile.
Transfer size (megabytes): 1
Online resource:
URL/service: http://dds.information.qld.gov.au/dds?title="CadastraldatafortnightlyextractFlindersLocalGovernmentArea"
Offline media: SHP or TAB
Transfer options:
Online resource:
URL/service: Function: download

## Metadata Reference Information

Hierarchy level (scope of the metadata): dataset
Identifier: flinders
Parent identifier: {7CDF9FFD-1259-454F-957A-87CE05A6AA42}
Metadata date stamp: 2010-08-10
Point of contact:
Organisation: Department of Natural Resources and Mines
Position: Senior Products Officer
Address:
Delivery point: QGIS Support
City: Brisbane
State: QLD
Postcode: 4000
Country: Australia
Email: Discovery@dnrm.qld.gov.au
Phone:
Voice: 61 7 33304440
Metadata Access Level:
Security classification (ISO 19115): unclassified
Use limitation: Public
Language: eng
Character set: utf8
Metadata standard name: ISO 19115:2005, ANZLIC ISO 1.1
Metadata version name: QGIS